{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["分项报价表"],"read":"whole","date_system":"1900"}

{"sheet":"分项报价表","index":0,"n_rows":13,"n_cols":8,"rows_kept":13,"merged":[[0,0,0,7],[10,0,10,5],[11,0,11,7],[12,0,12,7]]}
["谢岗一期提标滤布滤池系统设备委外维修采购项目分项报价表"]
["序号","采购项目","规格/服务/施工要求","数量","单位","所报不含税单价（元）","不含税小计（元）","备注"]
[1,"池壁承重板、“L”型承重钢板及“Ｈ”型承重钢构","材质为304#不锈钢，厚度10mm，适配现场滤布滤池，池壁承重板（尺寸：1300mm*1300mm，中心孔直径900mm）下方加装“L”型承重钢板（尺寸：1300mm*200mm）和“H”型承重钢构（尺寸：1500mm*200mm*2+500mm*200mm），分散池壁承重板承重力，确保安全。",1,"套",null,null,"/"]
[2,"支撑轮支架","与原尺寸一致的304#不锈钢支架，支架受力面增加加强筋，提高支架强度，钢板厚度10mm，支撑轮支架可拆卸方式安装，方便后续维修、更换。",3,"套",null,null,"每组滤布滤池成套设备3套支撑轮支架"]
[3,"支撑轮","高强度、耐腐蚀、耐磨损支撑轮（外径200mm，内径80mm，高120mm），材质为实心聚甲醛树脂（赛钢），支撑轮轴销与轴承配合小50个丝方便安装及日后维护保养。",3,"套",null,null,"每组滤布滤池成套设备3套支撑轮"]
[4,"支撑轮轴承","支撑轮轴承选用水下专用氧化锆陶瓷轴承（型号：6208），满足各种工况要求，如耐腐蚀、耐锈蚀、耐酸碱等。",6,"套",null,null,"每组滤布滤池成套设备6套支撑轮轴承"]
[5,"密封圈","硅胶密封圈（直径900mm），适配现场滤布滤池。",1,"套",null,null,"/"]
[6,"链条","材质为304#不锈钢链条定制作长度10米，厚度5MM。",1,"条",null,null,"定制"]
[7,"链轮","PE材质厚度50mm大的直径1200MM压轮张紧轮共计三件定制",1,"套",null,null,"定制,一套共计三件"]
[8,"技术服务费\n（措施费及管理费）","包含设备拆卸改造安装、现场制作、校准同心、安全管理、垃圾清理、调试等服务。",1,"项",null,null,"定制"]
["不含税合计（元）："]
["备注：\n1.当分项报价明细表内累计与报价表不符时，以报价表为准，修正分项报价明细表的各项报价。\n2.上述报价数值如需保留小数点后 2 位，从小数点后第 3 位四舍五入。"]
["                                                       报价人：（加盖公章）\n\n                                                                           日期：    年     月   日                                                                                                                                                                                         "]